MIDNITE SOLAR 1-63 AMP 150VDC DIN RAIL MOUNT SP BREAKER

Rated to break the full rated load at the rated voltage repeatedly (when mounted in a Midnite Solar enclosure), with NO DAMAGE. Always use a properly sized breaker for disconnecting. The breakers have been evaluated by ETL to 150VDC and are listed for US and Canada. All of the NRTL listings apply also, making them suitable for the solar industry.

* Environmental Rating - Type 1 (Indoor)
* DC Voltage Rating - 150VDC
* Wire Size Range - 14 to 6 AWG
* Width - .51 in (13mm)
* Number of poles - 1
* 10,000 AIC